Annual Vehicle Inspection Report	Ledger Road
Periodic inspection under 49 CFR 396.17. Components follow Appendix A to Part 396.	ledgerroad.com
	Motor carrier
	Carrier address
	Date of inspection

	Fleet unit no.
	Year and make
	Serial number (VIN)
	License plate and state
	Odometer

	☐ Tractor   ☐ Truck   ☐ Trailer   ☐ Bus   ☐ Other:
	Inspector’s name (print)



	Item
	OK
	Needs repair
	Repaired (date)
	
	Item
	OK
	Needs repair
	Repaired (date)

	1. BRAKE SYSTEM
	
	7. STEERING MECHANISM

	a. Service brakes
	☐
	☐
	
	
	a. Steering wheel free play
	☐
	☐
	

	b. Parking brake system
	☐
	☐
	
	
	b. Steering column
	☐
	☐
	

	c. Brake drums or rotors
	☐
	☐
	
	
	c. Front axle beam, steering components
	☐
	☐
	

	d. Brake hose
	☐
	☐
	
	
	d. Steering gear box
	☐
	☐
	

	e. Brake tubing
	☐
	☐
	
	
	e. Pitman arm
	☐
	☐
	

	f. Low pressure warning device
	☐
	☐
	
	
	f. Power steering
	☐
	☐
	

	g. Tractor protection valve
	☐
	☐
	
	
	g. Ball and socket joints
	☐
	☐
	

	h. Air compressor
	☐
	☐
	
	
	h. Tie rods and drag links
	☐
	☐
	

	i. Electric brakes
	☐
	☐
	
	
	i. Nuts
	☐
	☐
	

	j. Hydraulic brakes
	☐
	☐
	
	
	j. Steering system
	☐
	☐
	

	k. Vacuum systems
	☐
	☐
	
	
	8. SUSPENSION

	l. Antilock brake system
	☐
	☐
	
	
	a. U-bolts, spring hangers, axle parts
	☐
	☐
	

	m. Automatic brake adjusters
	☐
	☐
	
	
	b. Spring assembly
	☐
	☐
	

	2. COUPLING DEVICES
	
	c. Torque, radius or tracking components
	☐
	☐
	

	a. Fifth wheels
	☐
	☐
	
	
	9. FRAME

	b. Pintle hooks
	☐
	☐
	
	
	a. Frame members
	☐
	☐
	

	c. Drawbar/towbar eye
	☐
	☐
	
	
	b. Tire and wheel clearance
	☐
	☐
	

	d. Drawbar/towbar tongue
	☐
	☐
	
	
	c. Adjustable axle assemblies
	☐
	☐
	

	e. Safety devices
	☐
	☐
	
	
	10. TIRES

	f. Saddle-mounts
	☐
	☐
	
	
	a. Steering axle tires (power unit)
	☐
	☐
	

	3. EXHAUST SYSTEM
	
	b. All other tires
	☐
	☐
	

	a. Leaks near driver/sleeper compartment
	☐
	☐
	
	
	c. Speed-restricted tires
	☐
	☐
	

	b. Bus exhaust discharge point
	☐
	☐
	
	
	11. WHEELS AND RIMS

	c. Location near wiring or fuel supply
	☐
	☐
	
	
	a. Lock or side ring
	☐
	☐
	

	4. FUEL SYSTEM
	
	b. Wheels and rims
	☐
	☐
	

	a. Visible leak
	☐
	☐
	
	
	c. Fasteners
	☐
	☐
	

	b. Fuel tank filler cap
	☐
	☐
	
	
	d. Welds
	☐
	☐
	

	c. Fuel tank attachment
	☐
	☐
	
	
	12. Windshield glazing
	☐
	☐
	

	5. Lighting devices and reflectors
	☐
	☐
	
	
	13. Windshield wipers
	☐
	☐
	

	6. SAFE LOADING
	
	14. Motorcoach seats
	☐
	☐
	

	a. Load, spare tire and dunnage secure
	☐
	☐
	
	
	15. Rear impact guard
	☐
	☐
	

	b. Protection against shifting cargo
	☐
	☐
	
	
	

	c. Container securement devices
	☐
	☐
	
	
	


COMPONENTS NOT MEETING THE STANDARDS, AND REPAIRS MADE
	

	



	☐ This vehicle has passed an inspection in accordance with 49 CFR 396.17.
☐ The inspector meets the qualification requirements of 49 CFR 396.19.
I certify that this report is accurate and complete and complies with all the requirements of 49 CFR 396.21.


	Inspector’s signature
	Date


Each vehicle in a combination is inspected separately and must have passed within the preceding 12 months, with proof of the inspection on the vehicle (49 CFR 396.17). Keep this report for 14 months from its date, where the vehicle is housed or maintained (396.21(b)). Keep evidence of the inspector’s qualifications while they inspect for you and for one year after (396.19(b)).
