Pre-Trip Inspection Checklist	Ledger Road
A walk-around check for a truck or tractor and its trailer, covering the parts named in 49 CFR 392.7.	ledgerroad.com
	Carrier name
	Date
	Time

	Driver name
	Truck / tractor unit no.
	Trailer unit no.
	Odometer



	Item
	OK
	Defect
	
	Item
	OK
	Defect

	APPROACH AND ENGINE COMPARTMENT
	
	TRUCK OR TRACTOR

	Vehicle sits level; no leaks underneath
	☐
	☐
	
	Steer tires: tread, inflation, sidewalls
	☐
	☐

	Engine oil level
	☐
	☐
	
	Wheels, rims and lug nuts
	☐
	☐

	Coolant level and hoses
	☐
	☐
	
	Hub oil seals
	☐
	☐

	Power steering fluid
	☐
	☐
	
	Brake hoses, chambers and slack adjusters
	☐
	☐

	Belts
	☐
	☐
	
	Springs, air bags and shocks
	☐
	☐

	Windshield washer fluid
	☐
	☐
	
	Steering linkage
	☐
	☐

	IN THE CAB
	
	Fuel tank, cap and lines
	☐
	☐

	Gauges and warning lights
	☐
	☐
	
	Exhaust system
	☐
	☐

	Air pressure builds; low-air warning works
	☐
	☐
	
	Frame and driveshaft
	☐
	☐

	Parking brake holds
	☐
	☐
	
	Drive tires and wheels
	☐
	☐

	Service brakes
	☐
	☐
	
	Mud flaps
	☐
	☐

	Steering wheel free play
	☐
	☐
	
	COUPLING

	Horn
	☐
	☐
	
	Fifth wheel, locking jaws and release handle
	☐
	☐

	Windshield, wipers and washers
	☐
	☐
	
	Kingpin and apron
	☐
	☐

	Mirrors
	☐
	☐
	
	Air lines, glad hands and electrical cable
	☐
	☐

	Seat belt
	☐
	☐
	
	TRAILER

	Heater and defroster
	☐
	☐
	
	Landing gear raised, crank secured
	☐
	☐

	Emergency equipment: extinguisher, triangles, spare fuses
	☐
	☐
	
	Lights and reflectors
	☐
	☐

	LIGHTS AND REFLECTORS
	
	Tires, wheels and lug nuts
	☐
	☐

	Headlights, high and low beam
	☐
	☐
	
	Brakes and air lines
	☐
	☐

	Turn signals and four-way flashers
	☐
	☐
	
	Springs or air bags
	☐
	☐

	Brake lights and tail lights
	☐
	☐
	
	Doors, latches and seals
	☐
	☐

	Clearance and marker lights
	☐
	☐
	
	Rear impact guard
	☐
	☐

	Reflectors and conspicuity tape
	☐
	☐
	
	Cargo secured; tie-downs and tarps tight
	☐
	☐


DEFECTS FOUND
	

	

	



	Driver signature
	Last inspection report reviewed  ☐  Yes


Before driving, the driver must be satisfied that the vehicle is in safe operating condition and review the last driver vehicle inspection report (49 CFR 396.13), and that the parts and accessories listed in 392.7 are in good working order. Cargo must be properly distributed and adequately secured (392.9). A defect found on this check is reported on the driver vehicle inspection report (396.11).
