Driver Vehicle Inspection Report	Ledger Road
Items follow 49 CFR 396.11(a)(1).	ledgerroad.com

	Carrier name
	USDOT number
	Date
	Time

	Driver name
	Truck / tractor unit no.
	Trailer unit no.
	Odometer


INSPECTED ITEMS
	Item
	OK
	Defect
	Notes

	Service brakes, including trailer brake connections
	☐
	☐
	

	Parking brake
	☐
	☐
	

	Steering mechanism
	☐
	☐
	

	Lighting devices and reflectors
	☐
	☐
	

	Tires
	☐
	☐
	

	Horn
	☐
	☐
	

	Windshield wipers
	☐
	☐
	

	Rear vision mirrors
	☐
	☐
	

	Coupling devices
	☐
	☐
	

	Wheels and rims
	☐
	☐
	

	Emergency equipment
	☐
	☐
	

	Other (describe)
	☐
	☐
	


DEFECTS OR DEFICIENCIES FOUND
	

	

	



	Driver signature
	Co-driver signature (team operation)


REPAIR CERTIFICATION (CARRIER OR MECHANIC)
	☐ Defects listed above were repaired        ☐ Repair is unnecessary to operate safely


	Signature
	Date


NEXT DRIVER REVIEW
	Next driver signature
	Date


A driver who finds no defect or deficiency is not required to prepare a report (49 CFR 396.11(a)(2)). Some carriers require one anyway as company policy. When defects are reported, the carrier certifies repair or that repair is unnecessary before the vehicle is operated again (396.11(a)(3)), and the next driver reviews and signs the last report (396.13). Keep the original report, certification and next-driver review for three months (396.11(a)(4)).
